14252SB - PRESTO 1000 XL E - ECO type 4l - Adapted with rimless toilets bowls 
Concealed self-closing flush valves for rimless toilet bowl. Presto 1000 XL E ECO type 4l ref. 14252SB or technically equivalent. With an adjustable water volume of 4l, 60l/min flow regulator, a patented anti-blocking "S" system to avoid the water to flow continuously, an integrated stop valve, a 304L brushed stainless steel front with chrome brass push button, anti-siphonic device, self-cleaned ruby mechanism (or validated equivalent).

14252SB - PRESTO 1000 XL E - ECO type 4l - Adapted with rimless toilets bowls 
Concealed self-closing flush valves for rimless toilet bowl. Presto 1000 XL E ref. 14251SB or technically equivalent. Including:
- Adjustable water volume of 4l
- 60l/min flow regulator
- a patented anti-blocking "S" system to avoid the water to flow continuously
- an integrated stop valve
- a 304L brushed stainless steel front with chrome brass push button
- an anti-siphonic device
and a self-cleaned ruby mechanism. 
Included any suggestions for supplies and implementation. 
RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting