18460SB - Self-supporting mounting frame for direct Dual flush, Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL E DVA® dual volume direct flush valve. Presto 1000 XL E DVA®, ref 18460SB or technically equivalent. Volumes independently adjustable between 6l to 9l for large flush and 2.5l to 5l for small flush. 60l/min flow regulator. Self closing valve equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. Front plate made of brushed anti-fingerprint metal with double button for 2 different hunting volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device.  Epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution. 

18460SB - Self-supporting mounting frame for direct Dual flush, Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL E DVA® dual volume direct flush valve. Presto 1000 XL E DVA®, ref 18460SB or technically equivalent. Including:
- Volumes independently adjustable between 6l to 9l for large flush and 2.5l to 5l for small flush. 
- 60l/min flow regulator.
- Self closing valve equipped with a self-cleaning ruby mechanism 
- an S® safety system that prevents blockage in continuous flow.
- Front plate made of brushed anti-fingerprint metal with double button for 2 different hunting volumes.
- Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 
- Epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution. 
Included any suggestions for supplies and implementation.