18461SB - Self-supporting mounting frame for direct Dual flush - Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL A DVA® dual volume direct flush valve. Presto 1000 XL A DVA®, ref 18461SB or technically equivalent. Volumes independently adjustable between 6l to 9l for large flush and 2.5l to 5l for small flush. 60l/min flow regulator. Self closing valve equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. Bright chrome-plated front plate, anti-fingerprint metal with double button for 2 different hunting volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device.  Epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution. 

18461SB - Self-supporting mounting frame for direct Dual flush - Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL A DVA® dual volume direct flush valve. Presto 1000 XL A DVA®, ref 18461SB or technically equivalent. Including:
- Volumes independently adjustable between 6l to 9l for large flush and 2.5l to 5l for small flush. 
- 60l/min flow regulator. 
- Self closing valve equipped with a self-cleaning ruby mechanism 
- a S® safety system that prevents blockage in continuous flow. 
- Bright chrome-plated front plate, anti-fingerprint metal with double button for 2 different hunting volumes. 
- Integrated stop valve valve and anti-vacuum (anti-siphonic) device.  
- Epoxy coated steel frame with Galvanized legs and floor fixing plates. 
- Ready to use solution. 
Included any suggestions for supplies and implementation.