18493SB - Self-supporting mounting frame with PRESTO 7100 XL N - Suitable for rimless toilets bowls
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 7100 XL N direct flush valve. Presto 7100 XL N, ref. 18493SB or technically equivalent. With optoelectronic cell and push button equipped with a self-cleaning ruby mechanism, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. Water volume adjustable from 2 to 9l. 60l/min flow regulator. Automatic detection of the flow time according to the presence time (4/6l - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. 304L brushed stainless steel vandal-resistant front panel. Epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution. Comes with 1 PVC angle tube Ø 32 mm and 1 junction nozzle male 55 mm, 1 Extended straight PE tube 100 mm with adapter sleeve for connection to the bowl, 1 WC outlet angle PVC pipe dia. 100 mmand screw and dowel for toilet bowl fixing.

18493SB - Self-supporting mounting frame with PRESTO 7100 XL N - Suitable for rimless toilets bowls
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 7100 XL N direct flush valve. Presto 7100 XL N, ref. 18493SB or technically equivalent. Including:
- Optoelectronic cell and push button equipped with a self-cleaning ruby mechanism, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. 
- water volume adjustable from 2 to 9l
- 60l/min flow regulator
-automatic detection of the flow time according to the presence time (4/6l - short/long detection)
- a patented anti-blocking "S" system to avoid the water to flow continuously
- integrated stop valve and anti-siphonic device
- 304L brushed stainless steel vandal-resistant front panel
- epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution.
-  Comes with 1 PVC angle tube Ø 32 mm and 1 junction nozzle male 55 mm, 1 Extended straight PE tube 100 mm with adapter sleeve for connection to the bowl, 1 WC outlet angle PVC pipe dia. 100 mmand screw and dowel for toilet bowl fixing.
Included any suggestions for supplies and implementation.