18508SB - Self-supporting mounting frame for cross-partition control, for firewall, for rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL DVA direct dual flush valve. Presto 1000 XL DVA, ref. 18508SB or technically equivalent. With independently adjustable water volumes delivered from 6 to 9 liters (for high volume) adjustable with wrench, and from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate. 60l/min flow regulator. The self closing Flush valve is equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. The front plate is brushed chrome polished with double button for 2 different flush volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 
- Control plate and power tube of the bowl: As part of an appropriate installation, it allows to comply with the safety rules of a public receiving establishment (PRE), Article CO 31 of the order of June 25, 1980 modified which specifies that no degree of fire resistance is required for the ducts if their nominal diameter is less than or equal to 75 mm , provided the hole is not larger than the diameter of the duct or capillaries running through the wall
- In the event of integration into a fire-resistant partition, the support mounting frame is fitted with a connecting sleeve, a pipe and a reinforcement, all in NF Me (PVC B-s3, d0). As part of an appropriate installation, it complies with the Safety rules requirements of an establishment open to the public (ERP) article CO 31 of the order of June 25, 1980 amended for diameters less than or equal to 125mm. Refer to the instructions for detailed integration diagrams.
BE CAREFUL : This configuration is valid for maximum wall thickness 56mm (equivalent 2 BA13 + tiling for example)

18508SB - Self-supporting mounting frame for cross-partition control, for firewall, for rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL DVA direct dual flush valve. Presto 1000 XL DVA, ref. 18508SB or technically equivalent. Including:
- independently adjustable water volumes delivered from 6 to 9 liters (for high volume) adjustable with wrench, and from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate
- 60l/min flow regulator
- The self closing Flush valve is equipped with a self-cleaning ruby mechanism 
- a S® safety system that prevents blockage in continuous flow
- The front plate is brushed chrome polished with double button for 2 different flush volumes. 
- Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 
-  Control plate and power tube of the bowl: As part of an appropriate installation, it allows to comply with the safety rules of a public receiving establishment (PRE), Article CO 31 of the order of June 25, 1980 modified which specifies that no degree of fire resistance is required for the ducts if their nominal diameter is less than or equal to 75 mm , provided the hole is not larger than the diameter of the duct or capillaries running through the wall
- In the event of integration into a fire-resistant partition, the support mounting frame is fitted with a connecting sleeve, a pipe and a reinforcement, all in NF Me (PVC B-s3, d0). As part of an appropriate installation, it complies with the Safety rules requirements of an establishment open to the public (ERP) article CO 31 of the order of June 25, 1980 amended for diameters less than or equal to 125mm. Refer to the instructions for detailed integration diagrams.
BE CAREFUL : This configuration is valid for maximum wall thickness 56mm (equivalent 2 BA13 + tiling for example)