18524SB - Self-supporting mounting frame P1000 XL E DVA Eco 2l-4l - Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL E DVA ECO 2l-4l direct flush valve, ref 18524SB or technically equivalent.
With independently adjustable volumes from 4l for high flush to 2l for low flush. Flow regulator of 60l/min. Self closing valve equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. Front plate made of brushed anti-fingerprint metal with double button for 2 different hunting volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device.  Epoxy coated steel frame with Galvanized legs and floor fixing plates. Ready to use solution. Comes with 1 PVC angle tube Ø 32 mm and 1 junction nozzle male 50mm, 1 Extended straight PE tube 100 mm with adapter sleeve for connection to the bowl, 1 WC outlet angle PVC pipe dia. 100 mmand screw and dowel for toilet bowl fixing.

18524SB - Self-supporting mounting frame P1000 XL E DVA Eco 2l-4l - Adapted with rimless toilets bowls 
Self-supporting mounting frame for suspended rimless toilet bowl. Equipped with Preto 1000 XL E DVA ECO 2l-4l direct flush valve, ref 18524SB or technically equivalent. Including:
- independently adjustable volumes from 4l for high flush to 2l for low flush
- a flow regulator of 60l/min
- a self closing valve equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow
- a front plate made of brushed anti-fingerprint metal with double button for 2 different hunting volumes
- an integrated stop valve valve and anti-vacuum (anti-siphonic) device
- epoxy coated steel frame with galvanized legs and floor fixing plates
- ready to use solution
- comes with 1 PVC angle tube Ø 32 mm and 1 junction nozzle male 50mm, 1 Extended straight PE tube 100 mm with adapter sleeve for connection to the bowl, 1 WC outlet angle PVC pipe dia. 100 mm and screw and dowel for rimless toilet bowl fixing.
Included any suggestions for supplies and implementation.