18720SB - Kit PRESTO P1000 XL DVA for cross-partition control, for firewall, for rimless toilets bowls 
Flush valve for induct mounting (from 15 to 300mm) for rimless toilets bowls. Presto 1000 XL DVA, ref. 18720SB or technically equivalent. With independently adjustable water volumes delivered from 6 to 9 liters (for high volume) adjustable with wrench, and from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate. 60l/min flow regulator. The self closing Flush valve is equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. The front plate is brushed chrome polished with double button for 2 different flush volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device. Comes with 1 PVC flush tube and junction nozzle.
Solution of flush valve for induct mounting compliants with fire-resistant walls with the safety rules of a public receiving establishment (PRE), Article CO 31 of the order of June 25, 1980 for a maximum drilling of 75mm possible for the passage of the order. Access from the rear is mandatory for maintenance.

18720SB - Kit PRESTO P1000 XL DVA for cross-partition control, for firewall, for rimless toilets bowls 
Flush valve for induct mounting (from 15 to 300mm) for rimless toilets bowls. Presto 1000 XL DVA, ref. 18720SB or technically equivalent. Including:
- independently adjustable water volumes delivered from 6 to 9 liters (for high volume) adjustable with wrench, and from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate
- 60l/min flow regulator
- self closing flush valve is equipped with a self-cleaning ruby mechanism
-  a S® safety system that prevents blockage in continuous flow
- front plate is brushed chrome polished with double button for 2 different flush volumes
- integrated stop valve valve and anti-vacuum (anti-siphonic) device
- comes with 1 PVC flush tube and junction nozzle
Solution of flush valve for induct mounting compliants with fire-resistant walls with the safety rules of a public receiving establishment (PRE), Article CO 31 of the order of June 25, 1980 for a maximum drilling of 75mm possible for the passage of the order. Access from the rear is mandatory for maintenance.