27472 - Single electronic / sensor shower tap with battery and angle stop valve
Electronic single sensor shower panel for cold or premixed water. Presto type DL 400 E-SENSOR 27470 or technically equivalent. Hand detection Start / stop function. 30 sec flow time adjustable. Duty flush 30 sec 24h after last use (adjustable). Integrated 6V Battery power. Integrated flow regulator  (6 l/min or  8l/min). Top water inlet with angle stop valve. Fixed shower head with orientable jet and 42 anti-limescale spikes.

27472 - Single electronic / sensor shower tap with battery and angle stop valve
Electronic single sensor shower panel for cold or premixed water. Presto type DL 400 E-SENSOR 27470 or technically equivalent.
- Hand detection Start / stop function with 30 sec flow time adjustable
- Duty flush 30 sec 24h after last use (adjustable)
- Integrated 6V Battery power
- Integrated flow regulator  (6 l/min or 8l/min)
- Top water inlet 
- Delivered with angle stop valve
- Fixed shower head with orientable jet and 42 anti-limescale spikes