27475 - Single electronic / sensor shower tap with mains power supply and straight stop valve
Electronic single sensor shower panel for cold or premixed water. Presto type DL 400 E-SENSOR 27470 or technically equivalent. Hand detection Start / stop function. 30 sec flow time adjustable. Duty flush 30 sec 24h after last use (adjustable). 220 V / 7 V main power supply . Integrated flow regulator  (6 l/min or  8l/min). Top water inlet with straight stop valve. Fixed shower head with orientable jet and 42 anti-limescale spikes.

27475 - Single electronic / sensor shower tap with mains power supply and straight stop valve
Electronic single sensor shower panel for cold or premixed water. Presto type DL 400 E-SENSOR 27470 or technically equivalent.
- Hand detection Start / stop function with 30 sec flow time adjustable
- Duty flush 30 sec 24h after last use (adjustable)
- 220 V / 7 V main power supply
- Integrated flow regulator  (6 l/min or 8l/min)
- Top water inlet 
- Delivered with straight stop valve
- Fixed shower head with orientable jet and 42 anti-limescale spikes