31003 - PRESTO 12 - In-line water inlet
Self-Closing urinal valves NF certified G1/2" in-line supply.
Time flow: 6 seconds (± 2 sec.), Flow rate 9 l/min at 3 bar, 4 position flow internal adjustment device.
Equipped with a self-cleaning ruby mechanism and needle spring. Anti-water-hammering design.
Accessories to be provided according to ceramic, tube and nozzle.