55130 - Deck-mounted sensor mixer for washbasin with standard spout, rotating base, battery
Single lever mixer with electronic detection (CE), deck-mounted, with lateral temperature selector.
High swivel spout (236mm). Optoelectronic cell, 6 V lithium battery under basin.
Maximum temperature limitation adjustable, integrated flow limiter (6l/min -1 to 5 bar) cascade type.
Anti-lock system prohibits continuous flow, duty flush (30 seconds duty-flush, 72 hours after last/ use to avoid sleeping water).
PEX hoses G3/8" with integrated filter and check-valves, included stop valves.
10 year guarantee.
(Presto 5750 type ref. 55130 or technically equivalent)