55418SB - PRESTO 7100 XL N, mains power, 2L-4L - Adapted with rimless toilets bowls
Concealed sensor flush valve for rimless toilet bowl. Presto 7100 XL N, ref. 55418SB or technically equivalent. With optoelectronic cell aand push button equipped with a self-cleaning ruby mechanism, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. Water volume of 4l. 60l/min flow regulator. Automatic detection of the flow time according to the presence time (2/4L - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. 304L brushed stainless steel vandal-resistant front panel. 10 years guarantee

55418SB - PRESTO 7100 XL N, mains power, 2L-4L - Adapted with rimless toilets bowls
Concealed sensor flush valve for rimless toilet bowl. Presto 7100 XL N, ref. 55418SB or technically equivalent. 
- With optoelectronic cell and push button equipped with a self-cleaning ruby mechanism, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. 
- Water volume of 4l. 
-60l/min flow regulator. 
- Automatic detection of the flow time according to the presence time (2/4L - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously. 
- Integrated stop valve and anti-siphonic device.
- 304L brushed stainless steel vandal-resistant front panel.
- 10 years guarantee
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting