55418 - PRESTO 7100 XL N, mains power, 4L
Concealed sensor flush valve with optoelectronic cell and push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. Water volume 4 L. Constant flow rate of 1l/s from 1.2 bar to 4 bar. Automatic detection of the flow time according to the presence time (2/4L - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. 304L brushed stainless steel vandal-resistant front panel. 10 years guarantee

55418 - PRESTO 7100 XL N, mains power, 4L
Concealed sensor flush valve with optoelectronic cell and push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included.
- Water volume 4 L. 
- Constant flow rate of 1l/s from 1.2 bar to 4 bar.
- Automatic detection of the flow time according to the presence time (3/4L - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously. 
- Integrated stop valve and anti-siphonic device.
- 304L brushed stainless steel vandal-resistant front panel.
- 10 years guarantee