55434SB - PRESTO 7200 XL N, battery power - Adapted with rimless toilets bowls
Concealed sensor flush valve for rimless toilet bowl. Presto 7200 XL N, ref. 55434SB or technically equivalent. With optoelectronic cell and push button, Lithium battery operated (included).
Water volume adjustable from 2 to 9l. 60l/min flow regulator.
Automatic detection of the flow time according to the presence time(4/6L - short/long detection)
Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device.
304L brushed stainless steel vandal-resistant front panel.
10 years guarantee

55434SB - PRESTO 7200 XL N, battery power - Adapted with rimless toilets bowls
Concealed sensor flush valve for rimless toilets bowls. Presto 7200 XL N, ref. 55434SB or technically equivalent. Including:
- With optoelectronic cell 
- Push button, Lithium battery operated (included)
- Water volume adjustable from 2 to 9l
- 60l/min flow regulator
- Automatic detection of the flow time according to the presence time(4/6l - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously
- Integrated stop valve and anti-siphonic device
- 304L brushed stainless steel vandal-resistant front panel
-10 years guarantee
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting