55434 - PRESTO 7200 XL N, battery power
Concealed sensor flush valve with optoelectronic cell and push button, Lithium battery operated (included).
Water volume adjustable from 2 to 9 l. Constant flow rate of 1l/s from 1.2 bar to 4 bar.
Automatic detection of the flow time according to the presence time(4/6L - short/long detection)
Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device.
304L brushed stainless steel vandal-resistant front panel.
10 years guarantee

55434 - PRESTO 7200 XL N, battery power
Concealed sensor flush valve:
- With optoelectronic cell 
- Push button, Lithium battery operated (included)
- Water volume adjustable from 2 to 9 L
- Constant flow rate of 1l/s from 1.2 bar to 4 bar
- Automatic detection of the flow time according to the presence time(4/6L - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously
- Integrated stop valve and anti-siphonic device
- 304L brushed stainless steel vandal-resistant front panel
-10 years guarantee