55436SB - PRESTO 7300 XL N, mains power - Adapted with rimless toilets bowls 
Sensor flush valve for cross-partition for rimless toilets bowls. Presto 7300 XL N®  réf. 55436SB or technically equivalent. With optoelectronic cell and over-ride push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included.
Water volume adjustable from 2 to 9l. 60l/min flow regulator.
Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device.
304L brushed stainless steel vandal-resistant front panel.
10 year guarantee

55436SB - PRESTO 7300 XL N, mains power - Adapted with rimless toilets bowls 
Sensor flush valve for cross-partition for rimless toilets bowls. Presto 7300 XL N®  réf. 55436SB or technically equivalent. Including: 
- An optoelectronic cell and over-ride push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included.
- Water volume adjustable from 2 to 9l. 
- 60l/min flow regulator.
- Patented anti-blocking "S" system to avoid the water to flow continuously. 
- Integrated stop valve and anti-siphonic device.
- 304L brushed stainless steel vandal-resistant front panel.
- 10 year guarantee
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting