55436 - PRESTO 7300 XL N, mains power
Sensor flush valve for cross-partition with optoelectronic cell and over-ride push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included.
Water volume adjustable from 2 to 9 l. Constant flow rate of 1l/s from 1.2 bar to 4 bar.
Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device.
304L brushed stainless steel vandal-resistant front panel.
10 year guarantee