55450 - Single deck-mounted sensor tap - Main operated
Single tap Sensor operated (CE) with optoelectronic cell.
Mains supply by 230/7 Volt, transformer in IP65 waterproof housing.
Iintegrated flow regulator (8 l/min), anti-lock system preventing continuous flow. With filter and stop valve.
10 year guarantee.
(Presto SENSAO® type ref. 55450 or technically equivalent)