55476SB - PRESTO 7100 XL N,  mains power - Adapted with rimless toilets bowls
Concealed sensor flush valve for rimless toilet bowl. Presto 7100 XL N, ref. 55476SB or technically equivalent. With optoelectronic cell and push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included. Water volume adjustable from 2 to 9l. 60l/min flow regulator. Automatic detection of the flow time according to the presence time (4/6l - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. Anti-vandal stainless steel front plate with matte black coating and rose gold PVD button. 10 years guarantee

55476SB - PRESTO 7100 XL N,  mains power - Adapted with rimless toilets bowls
Concealed sensor flush valve forrimless toilets bowls. Presto 7100 XL N, ref. 55476SB or technically equivalent. Including:
- Optoelectronic cell and push button, with mains 7V via 12V / 24V AC or DC, compatible with 230 V AC / 12 V AC transformer not included
- Water volume adjustable from 2 to 9l
- 60l/min flow regulator
- Automatic detection of the flow time according to the presence time (4/6l - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously
- Integrated stop valve and anti-siphonic device
- Anti-vandal stainless steel front plate with matte black coating and rose gold PVD button
- 10 years guarantee
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting