55478SB - PRESTO 7200 XL N, battery power - Adapted with rimless toilets bowls 
Concealed sensor flush valve for wall-mounted rimless toilets bowls. Presto 7200 XL N®  réf. 55478SB or technically equivalent. With optoelectronic cell and push button, Lithium battery operated (included).
Water volume adjustable from 2 to 9l. 60l/min flow regulator. Automatic rinse. Automatic detection of the flow time according to the presence time(4/6l - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. Anti-vandal stainless steel front plate with matte black coating and rose gold PVD button. Delivered with a concealed box and an integrated stop valve. 10 years guarantee.

55478SB - PRESTO 7200 XL N, battery power - Adapted with rimless toilets bowls 
Concealed sensor flush valve for wall-mounted Rimless toilets bowl. Presto 7200 XL N® réf. 55478SB or technically equivalent. Including :
- With optoelectronic cell and push button 
- Lithium battery operated (included)
- Water volume adjustable from 2 to 9l
- 60l/min flow regulator.
- Automatic rinse
- Automatic detection of the flow time according to the presence time(4/6l - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously
- Integrated stop valve and anti-siphonic device
- Anti-vandal stainless steel front plate with matte black coating and rose gold PVD button
- Delivered with a concealed box and an integrated stop valve
- 10 years guarantee
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting