55478 - PRESTO 7200 XL N, battery power, black matte finishing
Concealed sensor flush valve Presto 7200 XL N®  réf. 55478 with optoelectronic cell and push button, Lithium battery operated (included).
Water volume adjustable from 2 to 9 L. Constant flow rate of 1l/s from 1.2 bar to 4 bar. Automatic rinse. Automatic detection of the flow time according to the presence time(6/9L - short/long detection). Patented anti-blocking "S" system to avoid the water to flow continuously. Integrated stop valve and anti-siphonic device. Anti-vandal stainless steel front plate with matte black coating and pink gold PVD button. Delivered with a concealed box and an integrated stop valve. 10 years guarantee.

55478 - PRESTO 7200 XL N, battery power, black matte finishing
Concealed sensor flush valve Presto 7200 XL N® réf. 55478:
- With optoelectronic cell
- Push button 
- Lithium battery operated (included)
- Water volume adjustable from 2 to 9 L
- Constant flow rate of 1l/s from 1.2 bar to 4 bar
- Automatic rinse
- Automatic detection of the flow time according to the presence time(6/9L - short/long detection)
- Patented anti-blocking "S" system to avoid the water to flow continuously
- Integrated stop valve and anti-siphonic device
- Anti-vandal stainless steel front plate with matte black coating and pink gold PVD button
- Delivered with a concealed box and an integrated stop valve
- 10 years guarantee