55480 - Concealed PRESTO SENSAO 8300N, battery power, black matte finishing
Concealed sensor urinal flush valve. Automatic flush by optoelectronic detection.  Solenoid valve will be automatically closed in case of low battery or any detector damage. 
Built-in M G 1/2'' (15x21) in-line inlet/outlet water. With integrated 6V-CRP2 lithium battery type in water-proof casing
Integrated in flush valve body. Anti-vandal stainless steel front plate with matte black coating. Automatic flow 24 hours after last use. Factory pre-setting flush program can be ajustable via PRESTO  programming tool (pre-rinse, flow duration, periodical flush et its duration). Delivered with a concealed box, washers, wall dowels and mounting screws,  an integrated stop valve and an instruction manual.

55480 - Concealed PRESTO SENSAO 8300N, battery power, black matte finishing
Concealed sensor urinal flush valve with:
- Automatic flush by optoelectronic detection
- Solenoid valve will be automatically closed in case of low battery or any detector damage
- Built-in M G 1/2'' (15x21) in-line inlet/outlet water
- With integrated 6V-CRP2 lithium battery type in water-proof casing
- Integrated in flush valve body
- Anti-vandal stainless steel front plate with matte black coating 
- Automatic flow 24 hours after last use
- Factory pre-setting flush program can be ajustable via PRESTO  programming tool (pre-rinse, flow duration, periodical flush et its duration)
- Delivered with a concealed box, washers, wall dowels and mounting screws,  an integrated stop valve and an instruction manual.