55482 - Concealed PRESTO SENSAO 8100N, mains power, black matte finishing
Concealed sensor urinal. Automatic flush by optoelectronic detection.  Solenoid valve will be automatically closed in case of power failure or any detector damage. Built-in M G 1/2'' (15x21) in-line inlet/outlet water. With mains 7V via 12V / 24V AC or DC , compatible with 230 V AC / 12 V AC transformer not included ( See Ref. 90464 / 90711/ 90610 / 90685 / 90704 / 90686). Integrated in flush valve body. Anti-vandal stainless steel front plate with matte black coating. Automatic flow 24 hours after last use. Factory pre-setting flush program can be ajustable via PRESTO  programming tool (pre-rinse, flow duration, periodical flush et its duration). Delivered with a concealed box, washers, wall dowels and mounting screws,  an integrated stop valve and an instruction manual.

55482 - Concealed PRESTO SENSAO 8100N, mains power, black matte finishing
Concealed sensor urinal with:
- Automatic flush by optoelectronic detection
- Solenoid valve will be automatically closed in case of power failure or any detector damage
- Built-in M G 1/2'' (15x21) in-line inlet/outlet water
- With mains 7V via 12V / 24V AC or DC , compatible with 230 V AC / 12 V AC transformer not included ( See Ref. 90464 / 90711/ 90610 / 90685 / 90704 / 90686)
- Integrated in flush valve body
- Anti-vandal stainless steel front plate with matte black coating 
- Automatic flow 24 hours after last use
- Factory pre-setting flush program can be ajustable via PRESTO  programming tool (pre-rinse, flow duration, periodical flush et its duration)
- Delivered with a concealed box, washers, wall dowels and mounting screws,  an integrated stop valve and an instruction manual.