56196 - Deck-mounted mixer sensor tap - Battery - Black and pink gold cover
Electronic Mixer SO'O range, with  detection (CE), deck-mounted.
Optoelectronic cell, 6 V lithium battery integrated.
Integrated flow limiter (3 l/min -1 to 5 bar) spray type.
Anti-lock system prohibits continuous flow. PEX hose G3/8" with integrated filter and check-valves, included stop valves.
Black body and pink gold cover finish.
3 year guarantee.
(Presto SO'O type ref. 56200 or technically equivalent)

56196 - Deck-mounted mixer sensor tap - Battery - Black and pink gold cover
- Electronic Mixer SO'O range, with  detection (CE), deck-mounted.
- Optoelectronic cell
- 6 V lithium battery integrated.
- Integrated flow limiter (3 l/min -1 to 5 bar) spray type.
- Anti-lock system prohibits continuous flow
- PEX hose G3/8" with integrated filter and check-valves, included stop valves.
- Black body and pink gold cover finish.
- 3 year guarantee.
- (Presto SO'O type ref. 56200 or technically equivalent)