57100 - Wall-mounted single sensor tap, all-integrated, battery, 3l/min
Sensor wall-mounted built-in single tap for washbasin Presto LINEA® ref 57100 or technically equivalent. With integrated flow regulator (3l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 1/2" connection (15x21), integrated stop valve, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Lead-free brass and chrome finish. Delivered with wall rose, filter gasket, self-adhesive sticker 

57100 - Wall-mounted single sensor tap, all-integrated, battery, 3l/min
Sensor wall-mounted built-in single tap for washbasin Presto LINEA® ref 57100 or technically equivalent. With :
- Integrated flow regulator (3l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 1/2" connection (15x21)
- Integrated stop valve
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Lead-free brass and chrome finish.
- Delivered with wall rose, filter gasket, self-adhesive sticker