57102 - Wall-mounted single sensor tap, all-integrated, battery, 1,9l/min Chrome
Sensor wall-mounted built-in single tap for washbasin Presto LINEA® ref 57102 or technically equivalent. With integrated flow regulator (1,9l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 1/2" connection (15x21), integrated stop valve, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome finish. Delivered with wall rose, filter gasket, self-adhesive sticker 

57102 - Wall-mounted single sensor tap, all-integrated, battery, 1,9l/min Chrome
Sensor wall-mounted built-in single tap for washbasin Presto LINEA® ref 57102 or technically equivalent. With :
- Integrated flow regulator (1,9l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 1/2" connection (15x21)
- Integrated stop valve
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish 
- Delivered with wall rose, filter gasket, self-adhesive sticker