57104 - Wall-mounted sensor mixer, cross-partition, mains 230V, 3l/min
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57104 or technically equivalent. With integrated flow regulator (3l/min), mains-operated with 230 V AC / 7 V DC Transformer, integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, M M G 3/8" (12x17) stop valves, Self-adhesive sticker, Extension cord 1m for transformer

57104 - Wall-mounted sensor mixer, cross-partition, mains 230V, 3l/min
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57104 or technically equivalent. With :
- Integrated flow regulator (3l/min) 
- Mains-operated with 230 V AC / 7 V DC Transformer
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish 
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, M M G 3/8" (12x17) stop valves, Self-adhesive sticker, Extension cord 1m for transformer