57106NM - Wall-mounted sensor mixer, cross-partition, Battery, 3l/min, black mat
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57106NM or technically equivalent. With integrated flow regulator (3l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Black mat finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, M M G 3/8" (12x17) stop valves, Self-adhesive sticker

57106NM - Wall-mounted sensor mixer, cross-partition, Battery, 3l/min, black mat
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57106NM or technically equivalent. With :
- Integrated flow regulator (3l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Black mat
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, M M G 3/8" (12x17) stop valves, Self-adhesive sticker