57108 - Wall-mounted sensor mixer, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57108 or technically equivalent. With integrated flow regulator (1,9l/min), Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided), integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker, Extension cord 1m for power supply

57108 - Wall-mounted sensor mixer, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57108 or technically equivalent. With :
- Integrated flow regulator (1,9l/min) 
- Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided)
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish 
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker, Extension cord 1m for power supply