57110 - Wall-mounted sensor mixer, cross-partition, Battery, 1,9l/min without stop valve
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57110 or technically equivalent. With integrated flow regulator (1,9l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker

57110 - Wall-mounted sensor mixer, cross-partition, Battery, 1,9l/min without stop valve
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57110 or technically equivalent. With :
- Integrated flow regulator (1,9l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish 
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker