57112CB - Wall-mounted single sensor tap, cross-partition,  mains 230V, 3l/min Brushed Copper
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57112CB or technically equivalent. With integrated flow regulator (3l/min), mains-operated with 230 V AC / 7 V DC Transformer, integrated solenoid valve, G 3/8" (12x17) hoses connection,  tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Brushed Copper Finish. Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, M M G 3/8" (12x17) Stop valve, Self-adhesive sticker, Extension cord 1m for transformer

57112CB - Wall-mounted single sensor tap, cross-partition,  mains 230V, 3l/min Brushed Copper
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57112CB or technically equivalent. With :
- Integrated flow regulator (3l/min) 
- Mains-operated with 230 V AC / 7 V DC Transformer
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Brushed Copper Finish
- Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, M M G 3/8" (12x17) Stop valve, Self-adhesive sticker, Extension cord 1m for transformer