57114OB - Wall-mounted single sensor tap, cross-partition,  Battery, 3l/min Brushed Gold
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57114OB or technically equivalent. With integrated flow regulator (3l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 3/8" (12x17) hoses connection,  tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Brushed Gold Finish. Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, M M G 3/8" (12x17) Stop valve, Self-adhesive sticker.

57114OB - Wall-mounted single sensor tap, cross-partition,  Battery, 3l/min Brushed Gold
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57114OB or technically equivalent. With :
- Integrated flow regulator (3l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Brushed Gold Finish
- Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, M M G 3/8" (12x17) Stop valve, Self-adhesive sticker.