57116 - Wall-mounted single sensor tap, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57116 or technically equivalent. With integrated flow regulator (1,9l/min), Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided), integrated solenoid valve, G 3/8" (12x17) hoses connection,  tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome Finish. Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, Self-adhesive sticker, Extension cord 1m for power supply

57116 - Wall-mounted single sensor tap, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57116 or technically equivalent. With :
- Integrated flow regulator (1,9l/min)
- Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided)
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome Finish
- Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, Self-adhesive sticker, Extension cord 1m for power supply