57118 - Wall-mounted single sensor tap, cross-partition, Battery, 1,9l/min without stop valve
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57118 or technically equivalent. With integrated flow regulator (1,9l/min), Integrated 6V lithium battery, integrated solenoid valve, G 3/8" (12x17) hoses connection,  tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Chrome finish. Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, Self-adhesive sticker.

57118 - Wall-mounted single sensor tap, cross-partition, Battery, 1,9l/min without stop valve
Sensor wall-mounted cross-partition single tap for washbasin Presto LINEA® ref 57118 or technically equivalent. With :
- Integrated flow regulator (1,9l/min)
- Integrated 6V lithium battery
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish 
- Delivered with brass clamping nut, gasket, washer, wall rose, PEX Hoses with revolving nut and filter gasket, Self-adhesive sticker.