57136 - Wall-mounted sensor mixer, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57136 or technically equivalent. With integrated flow regulator (1,9l/min), Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided), integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Lead-free brass and chrome finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker, Extension cord 1m for power supply

57136 - Wall-mounted sensor mixer, cross-partition, Mains 12-24V, 1,9l/min without stop valve Chrome
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57136 or technically equivalent. With :
- Integrated flow regulator (1,9l/min) 
- Low voltage power supply (12-24V AC/DC) in IP65 waterproof external case (transformer unit not provided)
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Lead-free brass and chrome finish.
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker, Extension cord 1m for power supply