57138NP - Wall-mounted sensor mixer, cross-partition, Battery, 1,9l/min without stop valve Polished Black
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57138NP or technically equivalent. With integrated flow regulator (1,9l/min), integrated 3V CR123A lithium batteries, integrated solenoid valve, G 3/8" (12x17) hoses connection, tube diameter 44 mm. Anti-overflow security time set to 30 seconds preventing the water to flow continuously. 30 sec adjustable automatic rinsing every 24h after last use. Lead-free brass body and Polished Black finish. Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker

57138NP - Wall-mounted sensor mixer, cross-partition, Battery, 1,9l/min without stop valve Polished Black
Sensor wall-mounted cross-partition mixer tap for washbasin Presto LINEA® ref 57138NP or technically equivalent. With :
- Integrated flow regulator (1,9l/min) 
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- G 3/8" (12x17) hoses connection
- Tube diameter 44 mm 
- Anti-overflow security time set to 30 seconds preventing the water to flow continuously
- 30 sec adjustable automatic rinsing every 24h after last use
- Lead-free brass body and Polished Black finish.
- Delivered with Brass clamping nut, Gasket, Washer, wall rose, PEX Hoses with revolving nuts, NF check valves and filter gaskets, Self-adhesive sticker