57200 - Deck-mounted sensor single tap for washbasin, mains 230V, 3l/min with stop valve Chrome
Deck-mounted sensor single tap for washbasin Presto LINEA® ref 57200 or technically equivalent. Touchless trigger, suitable for PRM. Flow 3l/min with integrated regulated aerator. Mains-operated with 230 V AC / 7 V DC transformer. Integrated solenoid valve. F G 3/8" (12x17) hose connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Chrome finish. Delivered with PEX hose, filter gaskets, stop valve.

57200 - Deck-mounted sensor single tap for washbasin, mains 230V, 3l/min with stop valve Chrome
Deck-mounted sensor single tap for washbasin Presto LINEA® ref 57200 or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 3l/min with integrated regulated aerator
- Mains-operated with 230 V AC / 7 V DC transformer
- Integrated solenoid valve
- F G 3/8" (12x17) hose connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Chrome finish
- Delivered with PEX hose, filter gaskets, stop valve