57208OB - Deck-mounted sensor mixer tap for washbasin, mains 230V, 3l/min with stop valve Brushed Gold
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57208OB or technically equivalent. Touchless trigger, suitable for PRM.  Flow 3l/min with integrated regulated aerator. Mains-operated with 230 V AC / 7 V DC transformer. Integrated solenoid valve. F G 3/8" (12x17) hoses connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Brushed Gold Finish. Delivered with PEX hoses, NF check valves, filter gaskets, stop valves.

57208OB - Deck-mounted sensor mixer tap for washbasin, mains 230V, 3l/min with stop valve Brushed Gold
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57208OB or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 3l/min with integrated regulated aerator
- Mains-operated with 230 V AC / 7 V DC transformer
- Integrated solenoid valve
- F G 3/8" (12x17) hoses connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Brushed Gold Finish
- Delivered with PEX hoses, NF check valves, filter gaskets, stop valves