57210NP - Deck-mounted sensor mixer tap for washbasin, mains 12-24V, 1.9l/min without stop valve Polished Black
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57210NP or technically equivalent. Touchless trigger, suitable for PRM.  Flow 1.9l/min with integrated regulated flow spray. Mains-operated without transformer for low voltage power supply (12-24V AC/DC). Integrated solenoid valve. F G 3/8" (12x17) hoses connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Polished Black Finish. Delivered with PEX hoses, NF check valves, filter gaskets.

57210NP - Deck-mounted sensor mixer tap for washbasin, mains 12-24V, 1.9l/min without stop valve Polished Black
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57210NP or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 1.9l/min with integrated regulated flow spray
- Mains-operated without transformer for low voltage power supply (12-24V AC/DC)
- Integrated solenoid valve
- F G 3/8" (12x17) hoses connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Polished Black Finish
- Delivered with PEX hoses, NF check valves, filter gaskets