57212IB - Deck-mounted sensor mixer tap for washbasin, battery, 3l/min with stop valve Brushed Stainless Steel
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57212IB or technically equivalent. Touchless trigger, suitable for PRM.  Flow 3l/min with integrated regulated aerator. Integrated 3V CR123A lithium batteries. Integrated solenoid valve. F G 3/8" (12x17) hoses connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Brushed Stainless Steel finish. Delivered with PEX hoses, NF check valves, filter gaskets, stop valves.

57212IB - Deck-mounted sensor mixer tap for washbasin, battery, 3l/min with stop valve Brushed Stainless Steel
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57212IB or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 3l/min with integrated regulated aerator
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- F G 3/8" (12x17) hoses connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Brushed Stainless Steel finish
- Delivered with PEX hoses, NF check valves, filter gaskets, stop valves