57214NP - Deck-mounted sensor mixer tap for washbasin, battery, 1.9l/min without stop valve Polished Black
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57214NP or technically equivalent. Touchless trigger, suitable for PRM.  Flow 1.9l/min with integrated regulated flow spray. Integrated 3V CR123A lithium batteries. Integrated solenoid valve. F G 3/8" (12x17) hoses connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Polished Black finish. Delivered with PEX hoses, NF check valves, filter gaskets.

57214NP - Deck-mounted sensor mixer tap for washbasin, battery, 1.9l/min without stop valve Polished Black
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57214NP or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 1.9l/min with integrated regulated flow spray
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- F G 3/8" (12x17) hoses connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Polished Black finish
- Delivered with PEX hoses, NF check valves, filter gaskets