57214 - Deck-mounted sensor mixer tap for washbasin, battery, 1.9l/min without stop valve Chrome
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57214 or technically equivalent. Touchless trigger, suitable for PRM.  Flow 1.9l/min with integrated regulated flow spray. Integrated 3V CR123A lithium batteries. Integrated solenoid valve. F G 3/8" (12x17) hoses connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Chrome finish. Delivered with PEX hoses, NF check valves, filter gaskets.

57214 - Deck-mounted sensor mixer tap for washbasin, battery, 1.9l/min without stop valve Chrome
Deck-mounted sensor mixer tap for washbasin Presto LINEA® ref 57214 or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 1.9l/min with integrated regulated flow spray
- Integrated 3V CR123A lithium batteries
- Integrated solenoid valve
- F G 3/8" (12x17) hoses connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use
- Chrome finish
- Delivered with PEX hoses, NF check valves, filter gaskets