60529AV - 135° Angled rail - Diameter 32mm - With virucidal film
Lift bar for WC. Presto type ref. 60529AV or technically equivalent. With 135 ° angle, 3 fixing points. In white epoxy finish steel, diameter 32 mm and length 400 x 400 mm. With transparent COVERSAFE ™ virucidal film, and destruction of 99.9% of viruses and bacteria in 24 hours. Efficiency tested and validated for 4 years. Supplied with rosettes finishing clip. Adapted to mobility-reduced people.