68075 - Wall-mounted sensor and timed-flow mixer tap - 3l/min
Wall-mounted mixer sensor tap Presto SAFE® ref 68075 or technically equivalent. With detection cell and solenoid valve integrated. 9V Lithium battery delivered with the tap. G 3/8" connection, 7 sec adjustable flow time, integrated flow regulator (3l/min), 30 sec adjustable automatic rinsing every 24h after last use, chrome finish, temperature stop, PEX hoses, stop valves with filters gaskets

68075 - Wall-mounted sensor and timed-flow mixer tap - 3l/min
Wall-mounted mixer sensor tap Presto SAFE® ref 68075 or technically equivalent. Including :
- Detection cell
- Delivered 9V lithium battery
- Integrated solenoid valve. 
- G 3/8" connection, 
- 7 sec adjustable flow time, 
- Integrated flow regulator (3l/min), 
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish
- Temperature stop, 
- PEX hoses
- Stop valves with filters gaskets