70800 - Deck-mounted mixer – upward spout
Single-lever deck-mounted mixer with upward spout. Swivel spout, projection 250 mm, height under spout 276 mm, diameter 22 mm. Ceramic cartridge with flow rate 25L / min at 38°C at 3 bar. Anti-limescale star-shaped flow straightener. Supply by PEX hose - stainless steel braid G1 / 2 '' 660 mm -  withstands a temperature of 75 ° C for 30 minutes (in the context of thermal shock), integrated non-return valves NF. . Chromed brass body and spout. Compatible with an extension. Reference 70800, brand PRESTO or equivalent.

70800 - Deck-mounted mixer – upward spout
Single-lever deck-mounted mixer with upward spout Reference 70800, brand PRESTO or equivalent, comprising:
- Swivel spout, projection 250 mm, height under spout 276 mm, diameter 22 mm
- Ceramic cartridge with flow rate 25L / min at 38°C at 3 bar
- Anti-limescale star-shaped flow straightener
- Supply by PEX hose - stainless steel braid G1 / 2 '' 660 mm -  withstands a temperature of 75 ° C for 30 minutes (in the context of thermal shock)
- Integrated NF non-return valves
- Compatible with an extension
- Chromed brass body and spout