70804 - Wall-mounted mixer tap with 2 holes – upward spout
Wall-mounted mixer with upward spout. Swivel spout, projection 250 mm, height under spout 226 mm, diameter 22 mm. 1/4 turn ceramic head with flow rate of 81L / Min at 3 bar. Interchangeable anti-limescale flow straightener. Integrated NF check valves. Eccentric fittings M1 / 2 '' - M3 / 4 '' supplied with rosettes. Chromed brass body and spout. Reference 70804, brand PRESTO or equivalent.

70804 - Wall-mounted mixer tap with 2 holes – upward spout
Wall-mounted mixer with upward spout, Reference 70804, of the PRESTO brand or equivalent, comprising:
- Swivel spout, projection 250 mm, height under spout 226 mm, diameter 22 mm
- 1/4 turn ceramic head with flow rate of 81L / Min at 3 bar
- Anti-limescale flow straightener
- Integrated NF check valves
- M1 / 2 '' - M3 / 4 '' offset fittings supplied with rosettes
- Chromed brass body and spout