70806 - Wall-mounted mixer tap with 2 holes – downward spout
Wall-mounted mixer with downward spout. Swivel spout, projection 300 mm, height under body 182 mm, diameter 22 mm. 1/4 turn ceramic head with flow rate of 81L / min at 3 bar. Interchangeable anti-limescale star-shaped flow straightener. Eccentric fittings M1 / 2 '' M3 / 4 '' supplied with rosettes. Delivered with NF check valves and 2 filters. Chromed brass body and spout. Reference 70806, brand PRESTO or equivalent.

70806 - Wall-mounted mixer tap with 2 holes – downward spout
Wall-mounted mixer with downward spout Reference 70806, of the PRESTO brand or equivalent, comprising:
- Swivel spout, projection 300 mm, height under body 182 mm, diameter 22 mm
- 1/4 turn ceramic head with flow rate of 81L / min at 3 bar
- Interchangeable anti-limescale star-shaped flow straightener.
- M1 / 2 '' M3 / 4 '' offset fittings supplied with rosettes
- Chromed brass body and spout
- NF check valves
- 2 filters