70812 - Column – deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower. 1/4 turn ceramic head mixer with chromed brass column and body, flexible, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm. Black hand shower M1 / 2 '' with 2 jets adjustable by the user. Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C maximum. PEX hoses - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves. Body and column in chromed brass. Reference 70812 of PRESTO brand or equivalent.

70812 - Column – deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower, Reference 70812 of PRESTO brand or equivalent, including:
- 1/4 turn ceramic head mixer with chromed brass column and body, flexible, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm
- Black M1 / 2 '' hand shower with 2 jets adjustable by the user. Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C maximum.
- PEX hoses - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves.
- Body and column in chromed brass