70814 - Wall-mounted column with 2 holes– rinsing head
2-hole wall-mounted  column with hand shower. 1/4 turn ceramic head mixer with chromed brass body and column, flexible hose, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm. Black M1 / 2 '' hand shower with 2 adjustable jets. Eccentric fittings M1 / 2 '' M3 / 4 '' supplied with rosettes. Integrated NF check valves. Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C maximum. Reference 70814, brand PRESTO or equivalent.

70814 - Wall-mounted column with 2 holes– rinsing head
Two-hole wall mounted column with hand shower, Reference 70814, brand PRESTO or equivalent, comprising:
- 1/4 turn ceramic head mixer with chromed brass body and column, flexible, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm
- Black M1 / 2 '' hand shower with 2 adjustable jets
- M1 / 2 '' M3 / 4 '' offset fittings supplied with rosettes. Integrated NF check valves
- Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C maximum