70818 - Column –deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower and filling spout. Single-lever mixer with ceramic cartridge with flow rate 20L / min at 3 bar, with chromed brass body and column, flexible, stainless steel spring and wall mounting bracket, can be cut between 60 and 200 mm. Black 1/2 '' MG hand shower with 2 adjustable jets, integrated non-return valve. Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max. Projecting spout 290 mm, height under spout 278 mm. PEX hoses - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves. Reference 70818, brand PRESTO or equivalent.

70818 - Column –deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower and filling spout, Reference 70818, brand PRESTO or equivalent, comprising:
- Single-lever mixer with ceramic cartridge with flow rate 20L /min at 3 bar, with body and column in chromed brass, flexible, stainless steel spring and wall mounting bracket, can be cut between 60 and 200 mm
- MG 1/2 '' black hand shower with 2 adjustable jets, integrated non-return valve.
- Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 °C. Continuous operating temperature at 70 °C max.
- Projecting spout 290 mm, height under spout 278 mm.
- PEX hoses - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves.